A Profils Ashok Gopalarathnam/Selig - "New" KR2S Airfoil     
AS 5046 16.00 % The AS5046 will work on stock spars.  
AS 5048 18.00 % I'd highly recommend using the AS5048 (18%) airfoil at the root, 
AS 5045 15.00 % while using the AS5045 (16%) at the tip. 


 
C Airfoils C  
Cap21 15.00 % CAP 21 airfoil 
CJ25209 09.50 % ?? 
 
 

 
D  Mark Drela airfoils 
Allegro  Set of 6 airfoils from the Allegro 2m 
ApogeeHLG  Set of 7 airfoils from the ApogeeHLG 

 
dd928416 08.40 % Delft sailplane  


 
E Eppler airfoils 
EB 380 10.00 %   Profil hybride étudié à partir des E 374 et E387 
E193g.U-K24 10.00 % Profil modifié pour intrados plat etudié pour volet à 24%  

 
 Airfoils EH by John Yost 
EH 19-17 07.00 % for swept wing tailless aircraft  

 
Elina 09.50 % ??  


 
F Airfoils F  
F4FRAS15 15.00 % Airfoil for "le Pou du ciel par" (c) Richard Fraser 

 

 
H Hannes Delago airfoils (Team Ariane)           
HD45 07.50 % "For fast models (F5B, F5D, slope)." 
HD 46 07.00 % "For fast models (F5B, F5D, slope)." 
HD 47 06.50 % "For fast models (z.B. F5B, F5D, slope). Ariane V10 wing airfoil." 
HD48 08.00 % "Optimized for F3B." 
HD 48A 08.50 % "Optimized for F3B." 
HD 48B 09.00 % "Optimized for F3B." 
HD 50 08.00 % "Special purpose F5B airfoil,  for the Ariane V5 and Ariane V6." 
HD 53 07.50 % "Special purpose F5B airfoil,  for the Ariane V7." 
HD 54 07.00 % "Special purpose S8E rocket glider airfoil,  for the Ariane RAK2." 
HD 800 08.00 % "General purpose tail airfoil." 
HD 801 07.00 % "General purpose tail airfoil, used on almost every Ariane plane." 

 


 

 Norbert Habe airfoils                                   
HLG
 HN-1027   HN-1029   HN-1033    HN-1033A 


 
F3F, F3B
 HN-163   HN-163TA   HN-163TB    HN-184   HN-211   HN-216    
HN-216TA   HN-321   HN-350    HN-352   HN-354  HN-354A    HN-354E 
HN 380   HN-436   HN-446    HN-462   HN-464   HN-785    HN-1038 


 
F3J
 HN-217   HN227   HN-239   HN333   HN350M01    HN350M02 
HN-354SM   HN-354OC   HN-360    HN-465   HN973 


 
Glider >3.5m
 HN-003   HN-188   HN-203    HN-304   HN-304TA   HN-309    HN-319 
HN-409   HN-411   HN-832   HN-832TA   HN-951   HN-956    HN-971 
HN-972   HN-1023 


 
Tailplane
 HN-153S   HN-274S   HN-275S    HN-276SA   HN-311S   HN-312S   
HN-315S   HN-316S 


 
Glider
 HN-184M   HN-418   HN-424    HN-450S   HN-961SA 
HN-1036   HN-1051   HN-1054 
  Up
 

 
 Horten airfoils 
standard 13.00 % From Modèle Magazine N° 489 06/ 1992 Mini Horten  B. Jarril 
Tropfen II 10.00 % Without vertical stabilizer, Washout 10°. 

 
 Helmut Quabeck airfoils 
HQW 1/9 08.94 %  
HQW2/8 08.00 % Used on F3B sailplane of Ph. Genvrin / F. Legou (France) 
HQW 3/10 10.00% Use on sailplane Soarmaster from GRAUPNER 

 
J Jedelski airfoils 
EJ 1 13.00 %  
EJ 85 see
 Typical airfoils 


 
M  Marcel Guwang airfoils Use on AEROMOD models 
Use this airfoils with flaps at 30% chord. 
MG 05 09.00 % Used on wing and tail of Voltij, tail of Miraj 
MG 06 07.40 % Used on  Prodij and on wing of Miraj 
MG 08 08.70 % Used on Avantaj and Essoraj 


 
   
 Martin Hepperle airfoils                                     
MH18B 11.80 % "for pylon racing model aircraft (Quickie 500)." 
MH23 08.01 % "for pylon racing model aircraft (FAI class F3D)." 
MH24 09.01% "for pylon racing model aircraft (FAI class F3D)." 
MH25 09.98 % "for pylon racing model aircraft (FAI class F3D)." 
MH26 10.99 % "for pylon racing model aircraft (FAI class F3D)." 
MH27 11.99 % "for pylon racing model aircraft (FAI class F3D)." 
MH31 07.99 % "for electric powered pylon racing and for F5B models." 
MH33 07.28 % "for electric powered pylon racing . also be used for F3B and F3J." 
MH34 08.51 % "for electric powered pylon racing and for F5B models." 
MH44 09.66 % "for allround RC-gliders ).Has been used on the sailplane Wizard." 
MH46 11.40 % "Low moment coefficient airfoil for tailless model aircraft." 
MH49 10.50 % "Low moment coefficient airfoil for tailless model aircraft." 
MH64 08.61 % "Low moment coefficient airfoil for tailless model aircraft." 
MH78 14.40 % "Low moment coefficient airfoil for tailless model aircraft." 
MH91 15.00 % "for man carrying hang gliders." 
MH92 15.50 % "for man carrying hang gliders." 
MH93 16.00 % "for man carrying hang gliders." 

 
 E. Molfino Airfoils                                                          
F5B fast airfoils
 MB714  MB7136  MC813  MD814  MD8135   Mjp712  Msa812 
All round F3B airfoils
 Mve8516  Mve8516flap 80% +3°  
Flying Wing airfoils
 Mjz1211  Mjp711flap 75% -3°  
   


 
N NACA Symmetrical airfoils                                       
Naca  0007 07.00 %  
Naca  0008 08.00 %  
Naca  0009 09.00 %  
Naca  0010 10.00 %  
Naca  0011 11.00 %  
Naca  0012 12.00 %  
Naca  0013 13.00 %  
Naca  0014 14.00 %  
Naca  0015 15.00%  


 NACA airfoils 
Naca 1410 10.00 %  
Naca 23009 09.00 %  
Naca 23015 15.00 %  
Naca 2412 12.00 %  
Naca 2413 13.00 %  
Naca 2415 15.00 %  
Naca 4412 12.00 %  
Naca 4415 15.00 %  
Naca 6409 09.00 %  
Naca 64A410 10.00 %  
Naca 63A612 12.00 % Up
 

 
R Ritz airfoils 
Ritz 1-30-10 10.00 %  
Ritz 1-30-12 12.00 %  
Ritz 2-30-10 10.00 %  
Ritz 2-30-12 12.00 %  
Ritz 3-30-10 10.00 %  
Ritz 3-30-12 12.00 %  
Ritz 3-30-15 15.00 %  

 
RS001 10.00 % ??  
RS001m05 10.00 % ??  
RS001T10 10.00 % ??  
RS004a 09.00 % ??  
 

 
S Serge Barth airfoils                                                    
SB95 11.5/2 11.50 % "Ces 3 profils sont utilisés en évolution de l'emplanture vers le saumon." 
SB95 10.5/2 10.50 % 
SB95 9.5/2 09.50% 
   
SB96 LM 08.00 % "Gratteur, pénétrant et assez facile à réaliser en structure..." 
SB96 MU 08.50 % "Très bon en F3F le MU(tant) gratte aussi facilement avec 2° de volets." 
   
SB96V 09.35 % Profil d'emplanture pour planeur de voltige. 
SB96VS 09.75 % Profil de saumon pour planeur de voltige. 
   
SB96 12.7/3 12.70 % "Cette évolution se caractérise par un Cz maxi très élevé tout en conservant une bonne finesse." 
SB96 11.6/3 11.60 % 
SB96 10.5 10.50 % 
   
SB97 EP 09.20 % "Ce profil, alternative au RG12A, excelle en gratte et vitesse." 
SB97 FW 08.83 % "Le FW se caractérise par un Cm0 pratiquement nul et un bon Cz max." 
SB97 8/1.25 08.00 % "Adapté aux racers motorisés, ce profil permet de bonnes accélération et des virages serrés." 
SB97 EPW 08.00 % "Profil taillé pour le 60" mais qui a aussi été utilisé sur des 4m. Bon en gratte et en vitesse." 
   
SB98 F3J 08.00 % "Pour le plaisir de gratter avec un planeur fin" 
   
SB98VR5 12.00 % Emplanture Pour planeur de voltige. (Série de 3 profils utilisés sur l'AIR 100 d'Eric Poulain) 
SB98VM5 10.95 % Milieu 
SB98VS5 10.00 % Saumon 
   
SB99 F3J 09.00 % Nouveau profil de Serge Barth (d'aprés Looping Déc-Janv 2000) 
 

 
2032C 08.00 % ??  


 
  Questions, suggestions and new airfoils are welcome. 